TIMx\_CCIN是对定时器中断进行测试

触发定时器的CCIN事件后进入中断

打印信息如下：

**TEXT START**

**TIMx CC1 EVENT PASS**

**TIMx CC2 EVENT PASS**

**TIMx CC3 EVENT PASS**

**TIMx CC4 EVENT PASS**

**Exit interrupt and test ends**